==============================================
  Lantronix DeviceInstaller for
  --------------------------------------------
  Windows Server 2008 SP2 and later and Windows 7 SP1 and later
  --------------------------------------------
  Software Release Notes
  --------------------------------------------
  Version 4.4.0.4
  Monday, March 27, 2017
  Copyright (c) 2003-2013, Lantronix
==============================================

This document describes the Lantronix DeviceInstaller for
Windows software release.

This document is divided into the following sections:

o Description
o Requirements
o Installation
o Upgrade Instructions
o New Features
o Resolved Problems
o Known Problems
o Technical Support

Description
===========
    This utility provides users a single application, with a graphical 
    interface and utilizing Microsoft's .NET Framework, to access various
    configuration functions for Lantronix networking products. This makes it
    easy to perform initial setup, IP address assignment, firmware upgrades,
    and configuration changes.

Requirements
============
    The following items are required to run DeviceInstaller:

    1.  Windows
    2.  Microsoft .NET Framework v4.0.
    3.  Microsoft Internet Explorer 5.1, or later.
    4.  30MB free hard drive space.
    
    The "Internet Connection Firewall" must be disabled, or else 
    UDP Port 30718 must be available.  Otherwise, you will not be 
    able to detect or communicate with any devices on the network.
    To configure, go to the Control Panel, go to Network Settings, 
    select the corresponding network adapter, choose Properties, and
    go to the Advanced tab.

Installation
============
    The DeviceInstaller is distributed in a single image as a self-extracting
    executable. It is included on the CD packaged with the device server.

    1.	The application installation directory defaults to
        C:\Program Files\DeviceInstaller4.4, unless another folder is 
        selected during the installation process. 
    2.  A shortcut to this application is created on the Start/Programs menu. 
    3.  A log file of the installation can be found at 
        c:\Users\<current user>\Local Settings\Temp\DeviceInstaller_Install.log

    NOTE: The Microsoft .NET Framework 4.0 must be installed.  This comes
    installed on Windows 7 and above. If for some reason you received this setup
    utility without the .NET Framework, you can download it at the following URL:
    
    http://download.microsoft.com/download/9/5/A/95A9616B-7A37-4AF6-BC36-D6EA96C8DAAE/dotNetFx40_Full_x86_x64.exe

    All installations use Windows Installer 4.5, and can be downloaded at the following URL:

    https://download.microsoft.com/download/2/6/1/261fca42-22c0-4f91-9451-0e0f2e08356d/WindowsXP-KB942288-v3-x86.exe

Upgrade Instructions
====================
    1.  The installation of DeviceInstaller 4.3 will not uninstall
        DeviceInstaller 2.0, 3.x, 4.1, or 4.2.
        
    To uninstall the DeviceInstaller utility manually, follow these steps:

    1.  Select Settings->Control Panel from the taskbar Start menu.
    2.  Double click on the Add/Remove Programs icon.
    3.  Under the Install/Uninstall tab, select DeviceInstaller in the
        Software list and then click Add/Remove. Follow the prompts.
        (Note: DeviceInstaller was the default Program Folder specified in
        the installation process.)

New Features
============
Version 3.6
    1.  Now supports all subnets.
    2.  New IP assignment wizard designed to detect and correct PC & Network
        configuration issues during the IP assignment.
    3.  Built in TCP/IP tutorial.
    4.  Now supports XSDRIN units.

Version 3.6.0.5
    1.  Now supports the VDS100
    2.  Now supports the XP485
    3.  DeviceInstaller now supports Simplified Chinese.

Version 3.6.0.6
    1.  Certain names of devices shown in the main window of DeviceInstaller
        have been changed to reflect their dual nature (see Productinfobase.txt):
          Old Name                    New Name
          --------------------------- --------------------------------------
          IAP DF1 Multi-Master        UDS-10/Cobox-FL IAP DF1 Multi-Master
          IAP Modbus Bridge           UDS-10/Cobox-FL IAP Modbus Bridge
          IAP Standard Tunnel         UDS-10/Cobox-FL IAP Standard Tunnel
          DSTni-XPress DR             UDS100/XPress DR IAP
    
Version 4.0.0.0
    1.  DeviceInstaller is now organized as a tree view of devices on the
        network.
    2.  Configuration dialogs have been removed from this version of
        DeviceInstaller.  A Web Browser and a Telnet console has been
        embedded into DeviceInstaller for ease of connecting and 
        configuring a device using the Web interface or the Telnet
        interface provided by each device.

Version 4.0.0.4
    1.	Supports the WiPort and WiBox WPA.
    
Version 4.0.0.7
    1.	Supports the AR - XPort AR.
    2.  Supports the XA - XPort IAP.
    3.  Supports the WA - WiPort IAP.
    
Version 4.1.0.1
    1.  Japanese Language support added.
    2.  Added support for L1 - OneTouch (LifeScan).
    3.  Added support for N0 - Mitsubishi Projector-Controller.
    4.  Added support for 128k ROM files for the Micro-100, XPort-01,
        Xport-03 and XPort-485.
    5.  Added support for upgrading multiple devices at one time.
    6.  Setup records can be saved and sent to other devices.
    7.  If a ProductInfobase.txt file is in the directory where
        setup.exe is executed, then after installation this
        ProductInfobase.txt file will be copied to the application
        directory.
    8.  Added Customization Options in Tools menu.
    9.  Wait time for device reboots is now user customizable.
    10. ProductInfoBase.txt supports "EXTRA_TITLE", "IGNORE_LEGACY"
        and "IGNORE_UNKNOWNS".
    
Version 4.1.0.3
    1.  Supports the V2 - LTX110
    2.  Supports the R1 - XPress DR+
    3.  Supports the U3 - UDS1100
    4.	Supports the X4 - XPort-01 with 6.1 Firmware
    
Version 4.1.0.4
    1.  Supports the A2 - EDS4100
    2.  Supports the FX - WiPort NR
    
Version 4.1.0.6
    1.  Supports the rA - XPress DR+ Standard Tunneling
    
Version 4.1.0.7
    1.  Supports the UA - UDS1100-IAP
    2.  Supports the U4 - UDS2100
    
Version 4.1.0.8
    1.  Supports the D3 - SDS1101
    2.  Supports the D4 - SDS2101
    3.  Supports the W6 - WiPort BG
    4.  Supports the W7 - WiBox BG
    
Version 4.1.0.9
    1.  Supports the A3 - EDS32PR
    2.  Supports the A4 - EDS16PR
    3.  Supports the A5 - XPress I/O
    4.  Supports the IA - XPress DR+ Wireless
    
Version 4.2.0.0
    1.  Converted from dependence on .NET Framework 1.1 to .NET Framework 2.0.
    2.  The Product Information Base is now in XML format instead of plain text.
        Support for new devices will be based on this file instead of creating
        a new executable.
    3.  Added the Lantronix Product Information Base XML editor.  The latest
        PIBx file can be download via FTP from this editor.
    4.  In previous versions of DeviceInstaller, devices that are found and are not
        on the same network as the PC running DeviceInstaller, are marked as unreachable.
        Now, a new option has been added to allow the user to select this behavior, or
        to not have DeviceInstaller mark this device as unreachable.
    5.  Serial Recovery now has a persisten status mode to help in debugging
        recovery issues.
    6.  Selected devices can be excluded from the search results via the exclude
        toolbar button or the 'Device->Exclude Devices From Search Results' menu item.

Version 4.2.0.2
    1.  Added support for EDS PS series of devices.
    
Version 4.2.0.4
    1.  Added support for the Spider Duo (K2).
    2.  Added support for the XPort Pro (E5).
    3.  Added a user configurable value for Discovery timeout.  This can be
        found in Tools->Options.
    4.  Name of XPort-03 has been changed to XPort-03/04.
    
Version 4.2.0.5
    1.  Added device images.
    2.  Added support for EDS1100 and EDS2100.
    
Version 4.3.0.0
    1.  Added support for 64 bit OSes. Supported 64 bit OSes are:
        Windows Vista x64, Windows 7 x64, and Windows 2008 Server x64.
    2.  Support of Windows 2000 has been dropped.

Version 4.3.0.1
    1.  There is now a new directory for the lantronix.pibx file for 4.3 
        versions of Lantronix software.
    2.  Online help is now pure HTML and works with other browsers other
        than Internet Explorer.

Version 4.3.0.2
    1.  Support for PremierWave EN added.
        File CDM20802_Setup.exe is copied to the DeviceInstaller installation
        directory. This file can be used to install a driver which allows
        DeviceInstaller to perform serial recovery over USB with the
        PremierWave EN. Serial recovery over USB running at 920K can be up to
        10x faster than a serial port running at 115200. Please refer to the
        PremierWave User's Manual on how to implement this functionality.
    2.  Support for Micro125 added

Version 4.3.0.3
    1.  Support for PremierWave XN added.
    2.  Support for PremierWave XC added.
    3.  Support for EDS-MD added.
    4.  Moved the menu item "Tools->Advanced->Recover Firmware"
        to "Tools->Recover Firmware."
    5.  Made optimizations to DeviceInstaller that resulted in speeding up
        the launch of the program, sped up the Search function, and
        sped up several other common functions.
    6.  A program, dping.exe, was added to the installation directory.
        This program will repeatedly "ping" a device via the 0x77FE port
        by sending the 0xF6 command until the user presses Ctrl-C.
    7.  A program, dsearch.exe, was added to the installation directory.
        This program does a search for devices from the command line.
    8.  A program, dlisten.exe, was added to the installation directory.
        This program listens on port 0x77FE to diagnose if discovery 
        broadcasts are being sent from DI.

Version 4.3.0.5
    1.  Support for xPico added.

Version 4.3.0.6
    1.  Support for xSenso added.

Version 4.3.0.7
    1.  Support for xDirect added.

Version 4.3.0.8
    1.  Support for xPico-IAP added.
    2.  Support for xDirect-IAP added.
    3.  Support for XPort-05 added.
    4.  Support for PremierWave NR added.
    5.  Support for EDS2100 (Nuevo) added.
    6.  Support for XPort Pro (Nuevo) added.

Version 4.3.0.9
    1.  Support for Micro125-IAP added.
    2.  Changed name of XPort Pro-04 to XPort Pro Lx6

Version 4.4.0.0
    1.  All products that start with the uppercase letter X
        have been changed to the lowercase letter x. 

Version 4.4.0.1
    1.  Added support for the xPico Wi-Fi
    2.  Added support for the PremierWave SE1000

Version 4.4.0.2
    1.  Added support for the PremierWave 2050
    2.  Serial Recovery now works for the EDS MD
    3.  Fixed Various Bugs
    4.  Added support for the PremierWave UDS W2040
    5.  Added a loading circle for long running operations...
        Made the UI more responsive.
    6.  The xPico Wifi can now be queried for data via its Web API.
    7.  Added SLC devices: S8-SLC8008, SA-SLC8024, SB-SLC8032, SD-SLC8040, SE-SLC8048
    8.  Added xPress DR (-03) (XP) and renamed and changed family for DA, EA, and 3D devices.
    9.  Added SGX 5150 (Q4)

Version 4.4.0.4
    1.  Added Support for xPico110 (6X)
    2.  Added Support for SGX 3550 (Q5)

Resolved Problems
=================
Version 3.6.0.5
    1.  Configable Pins and Email Triggers were missing when displaying
        configuration for WiPort v5.6.
    2.  Encryption Key length was changed from 16 characters for 128 bits
        and 8 characters for 64 bits.  The new values are 26 and 13 for 
        128 and 64 bits, respectively.
    3.  DeviceInstaller crashed when changing baudrates on the Advanced tab
        on the Edit Port Dialog.
    
Version 3.6.0.6
    1.  Encryption Key is no longer displayed a clear text.
    2.  Disabling the Ad Hoc Network Creation will make the Ad Hoc Network
        Name, Ad Hoc Country, and Ad Hoc Network Channel inaccessible.
    3.  The following problem has been fixed: At the WEP encryption key
        you will see not the first 2 characters on 64 bit encryption.
        If you type in the encryption in Device Installer and push the apply
        and Ok button the WIPort is not found with the search function.
    4.  The following problem has been fixed: If you want to change the
        WEP encryption from 64 bit to 128 bit in Device Installer you get
        an error message : "Invalid Object"
    5.  DeviceInstaller now correctly requests and parses the RCR and SCR
        registers from selected devices.
    6.  DeviceInstaller now correctly handles baudrate selects for the XPort-03.
    7.  Fixed various Simplified Chinese inconsistencies.
    8.  VDS100 can now assign baudrates up to 230K.

Version 3.6.0.7B1
    1.  Fixed issue where devices that only supported baudrates of 115K and
        below would not allow the baudrate to be changed.  An error was presented
        to the user stating that a baudrate of 230K was not a supported baudrate.
        Even though 230K was not selected as the baudrate to be changed to.

Version 3.6.0.7B2
    1.  Fixed issued where under certain conditions, some VDS100s where
        reported having 2 ports.
        
Version 4.0.0.0
    1.  Fixed issues where the WiBox could not be recovered via a com port
        using the Advanced Recovery option.
        
Version 4.0.0.5
    1.  Fixed issue where changing the IP address on a device, that has RS485
        enabled for the serial protocol, will change the serial protocol back
        to RS232.
    
Version 4.1.0.1
    1.  Fixed crash of DeviceInstaller on startup when the PC has
        no physical serial ports.
    2.  Fixed recurring invalid reuse of Sockets.
    3.  Calulation of subnet mask sent to the device was incorrect.
    4.  Fixed the clrscrn command for the XPort AR for Telnet.
    5.  Cut and Paste in the telnet tab now works.
    
Version 4.1.0.2
    1.  Fixed issue where setting the IP address cleared the Telnet password.
    
Version 4.1.0.4
    1.  Fixed issue where send a setup record retrieved from a device
        that has a static address.  When sending this setup record to
        another device, that device's IP address was changed to the IP
        address in the setup record.

Version 4.1.0.6
    1.  An Exception occurred when searching and the
        "Activate logging during searching." checkbox was checked.
    
Version 4.2.0.1
    1.  Fixed issue with Serial Recovery of the XPort AR.

Version 4.2.0.2
    1.  Fixed the problem where the user could not save or cancel
        changes made to the Product Information Base (PIBX) via the
        update PIB download from Lantronix's FTP site.
        
Version 4.2.0.3
    1.  Fixed issue when running on Japanese Windows.  The Name, Group and Comments
        fields where uneditable in the Details Tab.
    
Version 4.2.0.4
    1.  Fixed an issue with the Add Device menu item.  Now devices that are added
        from another subnet than the PC running DI is, will correctly obtain
        configuration from the device.

Version 4.2.0.5
    1.  All interfaces on a NIC are now shown in the Options Form.
    2.  The cancel button is now enabled during IP Assignment.
    3.  The Add Device option now handles HostNames correctly.
    4.  Assigning an IP address to CoBOS devices inadvertently changed the
        Connect Mode of the device in certain situations. This issue has now
        been fixed in this version.
        
Version 4.3.0.1
    1.  Fixed issue where the NIC selection in the Options dialog did not display
        Network Interfaces in the PC did not have access to DNS.

Version 4.3.0.2
    1.  Fixed issue with the watchdog timer firing for EX chip devices during
        serial recovery.

Version 4.3.0.4
    1.  Fixed issue 

Version 4.3.0.4
    1.  Fixed issue with Serial Recovery failing on the PremierWave XC.

Version 4.3.0.5
    1.  Fixed issue with Serial Recovery failing on Evolution Devices such as
	    the EDS series of devices.

Version 4.4.0.0
    1.  xPort 03-04 (X2) Serial Recovery fixed.
    2.  Added xPort-IAP-05 (YM).
    3.  Change all "x" characters in the beginning of product names to lowercase.
        (ie. XPort to xPort)

Version 4.4.0.1
    1.  Fixed serial recovery issue with PremierWave XC HSPA+
    2.  Fixed serial recovery issue with CoBos devices with parallel flash.
    3.  Fixed serial recovery issue with xPico Wifi.

Known Problems
==============
    1.  Multiple devices cannot be upgraded at the same time.
    2.  Location of Custom Web Pages cannot be specified on the devices that
        support this feature.
    3.  If a device is set with DHCP enabled and AutoIP disabled and
        there is no DHCP server on the network, DeviceInstaller will not be
        able to discover the device.

Version 4.0.0.0
    1.  Some devices will not connect correctly via the embedded Web Browser.
        These devices need a different Java Virtual Machine.  Either use an
        external browser for these cases or perform the following tasks:
        
        1.	Load and install the latest Java JVM from www.java.com.
        2.	Add the environment variable "JAVA_PLUGIN_WEBCONTROL_ENABLE" with
            a value of "Sun5uxOrz".
    
Technical Support
=================
    If you have a question about the DeviceInstaller utility, first 
    look in the online Help file. When the program is running, press 
    the F1 key to automatically display Help, or select Contents in
    the Help pull-down menu. This Help file can also be accessed 
    via the shortcut on the Start/Program menu.

    If you cannot find an answer, please try our website at
    www.lantronix.com/support.  If you still cannot find an answer,
    please contact Lantronix technical support at
    1-800-422-7044 US or 1-949-453-7198.

Copyright (c) 2003-2006, Lantronix. All rights reserved.
Windows, .NET and Internet Explorer are trademarks of Microsoft Corporation.
Save Installation... Cancel Ctl-Alt-Sht-L 0 Forever
Ctl-Alt-Sht S Set Names
